09/23/2013

5-Dampling\_slides

MRAI: minimum route advertisement interval.

P6 Per prefix (in standard) vs. per neighbor (in implementation)

P9 half life: 最高penalty至中间penalty之时间。

P12 False damping is caused because:

BGP explores alternate paths during routing convergence.

….

muffling effect

Paper figure 8: no dampling means what?

Intended: calculated by mathematical model